**Food & Nutrition: Thermometer Calibration Log**

1. Fill glass with crushed ice, then add water to just below level of ice and stir;
2. Immerse thermometer stem into slush, keeping the stem away from bottom and sides;
3. Rotate nut under head until pointer reads 32°F;
4. Check calibration weekly and complete thermometer calibration log;
5. Clean and sanitize thermometer before use.

**MONTH/ YEAR: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | Reading | Calibrated by:  (INITIALS) | Total Number Tested |  | Single thermometer test | Number replaced |
| 1. |  |  |  |  |  |  |
| 2. |  |  |  |  |  |  |
| 3. |  |  |  |  |  |  |
| 4. |  |  |  |  |  |  |
| 5. |  |  |  |  |  |  |
| 6. |  |  |  |  |  |  |
| 7. |  |  |  |  |  |  |
| 8. |  |  |  |  |  |  |
| 9. |  |  |  |  |  |  |
| 10. |  |  |  |  |  |  |
| 11. |  |  |  |  |  |  |
| 12. |  |  |  |  |  |  |
| 13. |  |  |  |  |  |  |
| 14. |  |  |  |  |  |  |
| 15. |  |  |  |  |  |  |
| 16. |  |  |  |  |  |  |
| 17. |  |  |  |  |  |  |
| 18. |  |  |  |  |  |  |
| 19. |  |  |  |  |  |  |
| 20. |  |  |  |  |  |  |
| 21. |  |  |  |  |  |  |
| 22. |  |  |  |  |  |  |
| 23. |  |  |  |  |  |  |
| 24. |  |  |  |  |  |  |
| 25. |  |  |  |  |  |  |
| 26. |  |  |  |  |  |  |
| 27. |  |  |  |  |  |  |
| 28. |  |  |  |  |  |  |
| 29. |  |  |  |  |  |  |
| 30. |  |  |  |  |  |  |
| 31. |  |  |  |  |  |  |

**INSTRUCTIONS**: Calibrate all thermometers in use and at minimum perform weekly calibrations (check your facility policy).

* **For digital thermometers, please read manufacturer’s instructions**.
* For replacement thermometers, document calibration and check to indicate single thermometer test.